# Version 1.0 | 2023/02/23

* Initial release
  + CD74HC73E JK Flip Flop IC replaced CD4027BCN Dual Flip Flop IC.
  + 3D printed enclosure with Battery holder.
  + 3D Printed LED spacer added to simplify the assembly process
  + Added switch equipped jacks, allowing device to be turned on via plugging in.